#!/bin/sh
#
# k8temp
#
# Plugin to monitor the CPU temperature through lm-sensors
# on multicore AMD cpus 
#
# Author: Marc Schiffbauer <marc@schiffbauer.net>
#
# Requirements:
# 	- A configured lm-sensors installation with k8temp kernel module
#	- rewuired shell commands: sensors, grep, sed, uniq, cut
#
# Parameters supported:
#
# 	config
# 	autoconf
#
# Magic markers:
#%# capabilities=autoconf

# VERSION 1.0

case $1 in
	config)
		I=1
		LAST_CORE=""
		echo "graph_title CPU temperature"
		echo "graph_vlabel temperature in °C"
		echo "graph_options light"
		echo "graph_info This graph shows temperature of all CPU cores in °C"
		echo "graph_category sensors"
		sensors -uA | grep "^Core" | while read CORE FOO TEMP REST; do
			if [ "$LAST_CORE" == "$CORE" ]; then
				I=$((I+1))
			else
				I=1
			fi
			LAST_CORE=$CORE
			CORE_NUM=$(echo $CORE | sed 's/Core//')
			echo "core${CORE_NUM}_${I}.label Core ${CORE_NUM} sensor $I"
			#echo "core${CORE_NUM}_${I}.draw LINE1"
			echo "core${CORE_NUM}_${I}.warning 65"
			echo "core${CORE_NUM}_${I}.critical 80"
		done
        	exit 0
	;;
	autoconf)
	if [ "$(sensors -uA | grep "^Core" | uniq)" ]; then
                echo "yes"
                exit 0
        else
                echo "no"
                exit 1
        fi
esac
 
sensors -uA | grep "^Core" | while read CORE FOO TEMP REST; do
	if [ "$LAST_CORE" == "$CORE" ]; then
		I=$((I+1))
	else
		I=1
	fi
	LAST_CORE=$CORE
	CORE_NUM=$(echo $CORE | sed 's/Core//')
	TEMP=$(echo $TEMP | cut -d"." -f1)
	echo "core${CORE_NUM}_${I}.value $TEMP"
done
 
