#!/bin/sh
#
# Plugin to monitor harddrive temperatures through SMART.
#
# This plugin is an alternative to hddtemp_smartctl, which is
# the preferred one.
#
# client-conf.d/-options:
# 	
# 	drives		-- List drives to monitor. E.g. "hda hdc".
#
# $Log$
# Revision 1.4.2.1  2005/01/25 21:00:01  jimmyo
# Added plugin generic/hddtemp_smartctl, made by Lupe Christoph. Made it the default hddtemp plugin.
#
# Revision 1.4  2004/11/10 16:00:39  jimmyo
# Applied patch from Nicolas Stransky to generic/hddtemp, to fetch temp more elegantly (SF#1052845).
#
# Revision 1.3  2004/05/20 19:02:36  jimmyo
# Set categories on a bunch of plugins
#
# Revision 1.2  2004/01/29 19:39:00  jimmyo
# Generic plugins now use printf instead of echo -n, as this is more portable (SF#885564)
#
# Revision 1.1  2004/01/02 18:50:00  jimmyo
# Renamed occurrances of lrrd -> munin
#
# Revision 1.1.1.1  2004/01/02 15:18:07  jimmyo
# Import of LRRD CVS tree after renaming to Munin
#
# Revision 1.2  2003/12/18 19:16:00  jimmyo
# Changes from Alexandre
#
# Revision 1.1  2003/12/18 19:04:37  jimmyo
# New plugin: Alexandre Dupouy contributed "hddtemp".
#
#
#%# family=contrib

hddtemp=${hddtemp:-/usr/sbin/hddtemp}

if [ "$1" = "autoconf" ]; then
        if [ -x "$hddtemp" ]; then
                echo yes
                exit 0
        else
                echo no
                exit 1
        fi
fi

if [ "$1" = "config" ]; then

        echo 'graph_title HDD temperature'
        echo 'graph_args --base 1000 -l 0'
        echo 'graph_vlabel temp in °C'
        echo 'graph_category sensors'
        for a in $drives ; do echo $a.label $a `$hddtemp -q /dev/$a | cut -d: -f 2` ; done
        exit 0
fi

for a in $drives ; do printf "$a.value $($hddtemp -n -q /dev/$a)\n" ; done
